{"text_format":"2","workbook":"xls","n_sheets":2,"sheets":["4. Gang 1000-3000 mit LMM","4. Gang 1000-3000 mit Diode"],"not_rendered":{"charts":4,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"4. Gang 1000-3000 mit LMM","index":0,"n_rows":22,"n_cols":13,"rows_kept":22,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["Wednesday,28,February,2007,15:13:27"]
["038 906 019 KD ",null,"1.9l R4 EDC 0400SG  4897"]
[]
[null,"Group A:","'008",null,null,null,"Group B:","'011",null,null,null,"Group C:"," Not Running"]
[null,null,"Engine speed","IQ driver's req","IQ via rpm(Torq)","IQ via MAF",null,"Engine speed","Spec. intake press.","Actual intake press.","D.cycle MAP"]
[null,"TIME","2850-3150","65-70","47-51","47-60","TIME","2850-3150","2200-2400","2100-2600","35-80%","TIME"]
["MARKER","STAMP"," /min"," mg/R"," mg/R"," mg/R","STAMP"," /min",null,null," %","STAMP"]
[null,0.78,1176,69.7,37.1,29.1,0.38,1134,1524,1104,19.9]
[null,1.58,1239,69.7,39.5,31,1.18,1218,1632,1200,19.9]
[null,2.38,1323,69.7,42,33.8,1.98,1281,1728,1296,19.9]
[null,3.18,1407,69.7,45,41.7,2.78,1365,1800,1428,19.9]
[null,3.98,1533,69.7,48.6,51.9,3.58,1470,1908,1680,30.7]
[null,4.78,1680,69.7,52.2,57.1,4.38,1617,2040,2028,47]
[null,5.58,1848,69.7,55.2,57.6,5.18,1764,2172,2304,56.6]
[null,6.38,2037,69.7,54.9,57.9,5.98,1932,2244,2340,60.6]
[null,7.18,2184,69.7,53.8,57.6,6.78,2121,2292,2280,59.8]
[null,7.98,2352,69.7,53,57.4,7.58,2268,2316,2220,57.4]
[null,8.78,2499,69.7,52.4,57.4,8.38,2436,2328,2220,57.8]
[null,9.58,2646,69.2,51.9,56.8,9.18,2583,2340,2292,58.6]
[null,10.38,2793,68.6,51.3,56.5,9.98,2730,2340,2340,62.2]
[null,11.18,2940,68.1,51.1,56,10.78,2877,2340,2352,64.5]
[null,11.98,3087,67.5,50.5,55.7,11.58,3003,2340,2328,64.5]

{"sheet":"4. Gang 1000-3000 mit Diode","index":1,"n_rows":24,"n_cols":13,"rows_kept":24,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["Wednesday,28,February,2007,15:18:42"]
["038 906 019 KD ",null,"1.9l R4 EDC 0400SG  4897"]
[]
[null,"Group A:","'008",null,null,null,"Group B:","'011",null,null,null,"Group C:"," Not Running"]
[null,null,"Engine speed","IQ driver's req","IQ via rpm(Torq)","IQ via MAF",null,"Engine speed","Spec. intake press.","Actual intake press.","D.cycle MAP"]
[null,"TIME","2850-3150","65-70","47-51","47-60","TIME","2850-3150","2200-2400","2100-2600","35-80%","TIME"]
["MARKER","STAMP"," /min"," mg/R"," mg/R"," mg/R","STAMP"," /min",null,null," %","STAMP"]
[null,0.38,1008,39.5,31,37.6,0.77,1050,1404,1068,19.9]
[null,1.18,1092,69.7,33.8,41.2,1.58,1134,1500,1140,19.9]
[null,1.98,1155,69.7,36.2,44.7,2.37,1176,1596,1224,21.9]
[null,2.77,1218,69.7,38.7,47.5,3.17,1260,1692,1320,19.9]
[null,3.57,1302,69.7,41.2,49.7,3.98,1344,1776,1488,20.3]
[null,4.38,1386,69.7,44.5,52.2,4.78,1449,1896,1728,29.5]
[null,5.18,1512,69.7,48,54.6,5.58,1575,2004,1980,45]
[null,5.98,1659,69.7,51.3,56.8,6.38,1743,2148,2256,54.2]
[null,6.78,1827,69.7,54.6,57.6,7.18,1890,2232,2328,57.8]
[null,7.58,1995,69.7,55.2,57.9,7.98,2058,2280,2292,59.8]
[null,8.38,2142,69.7,54.1,57.6,8.78,2226,2316,2244,59]
[null,9.18,2310,69.7,53,57.6,9.58,2394,2328,2196,56.6]
[null,9.98,2457,69.7,52.4,57.4,10.38,2541,2340,2268,58.6]
[null,10.78,2604,69.5,51.9,56.8,11.18,2688,2340,2328,60.6]
[null,11.58,2751,68.6,51.3,56.5,11.98,2835,2340,2352,63.4]
[null,12.38,2898,68.1,51.1,56.3,12.78,2961,2340,2340,63.8]
[null,13.18,3024,67.5,50.8,55.7,13.58,3087,2340,2316,64.1]