{"text_format":"2","workbook":"xls","n_sheets":3,"sheets":["Tabelle1","Tabelle2","Tabelle3"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Tabelle1","index":0,"n_rows":52,"n_cols":8,"rows_kept":52,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
[null,null,"6-Gang Getriebe"]
[null,"Ibiza alt","Ibiza FR"]
[null,"Polo EU3","Polo EU4","Golf syncro","Ibiza Cupra","Golf"]
["Motor / Getriebe","ASZ / FSM","BLT / HDS","ASZ / FEL","BPX / ?","ASZ / ERF"]
["Zylinder",4,4,4,4,4]
["1. Gang",3.769,3.769,3.769,3.357,3.769]
["2. Gang",2.087,2.087,2.087,2.087,2.087]
["3. Gang",1.324,1.324,1.324,1.469,1.324]
["4. Gang",0.911,0.977,0.911,1.088,0.977]
["5. Gang",0.902,0.975,0.902,1.108,0.975]
["6. Gang",0.756,0.814,0.756,0.912,0.814]
[]
["Achse 1 - 4",2.955,3.238,3.875,2.955,3.238]
["Achse 5 - 6",2.407,2.615,3.1,2.407,2.615]
[]
["Reifen Breite",195,195,195,205,195]
["Querschnitt",55,55,65,40,65]
["Zoll",15,15,15,17,15]
["Abrollumfang mm",1818.0615,1818.0615,1937.1285,1818.9773999999998,1937.1285,0,0]
[]
[null,null,"Geschwindigkeit km/h"]
["Gang      /      rpm",4000,4000,4000,4000,4000]
[1,39.17745217800033,35.75335737677301,31.832579190167674,44.00780609953592,38.09488707903018,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[2,70.75218843262255,64.56847338431118,57.48777717668516,70.78783185248784,68.79713914751544,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[3,111.52554173631665,101.77825071983192,90.61706266445766,100.56787275435133,108.44382885261687,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[4,162.08541960360398,137.92671847805266,131.6981240041075,135.78511495968942,146.95970255973873,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[5,200.97275407924224,171.13683777026034,166.26523138545167,163.690205612691,182.34479188115898,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[6,239.78495261835522,204.98577005651575,198.37465437788018,198.86924102945352,218.41053081588453,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[]
[]
[null,null,"Drehzahl-Schaltsprünge"]
["1 - 2",1.8059415428845234,1.8059415428845225,1.8059415428845227,1.6085289889793968,1.805941542884523,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
["2 - 3",1.5762839879154078,1.5762839879154082,1.5762839879154082,1.4206943498978895,1.576283987915408,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
["3 - 4",1.4533479692645441,1.3551688843398157,1.4533479692645443,1.3501838235294117,1.3551688843398157,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
["4 - 5",1.2399187698112581,1.240780899151836,1.262472283813747,1.2055092022515557,1.2407808991518359,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
["5 - 6",1.1931216931216935,1.1977886977886976,1.1931216931216932,1.2149122807017543,1.1977886977886978,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[]
[null,null,"Geschw. Erhöhung bis Ende nächster Gang (km/h)"]
["Start 1.Gang",39.17745217800033,35.75335737677301,31.832579190167674,44.00780609953592,38.09488707903018,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
["1 - 2",31.574736254622216,28.815116007538165,25.655197986517482,26.78002575295192,30.702252068485258,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
["2 - 3",40.77335330369411,37.20977733552074,33.129285487772506,29.780040901863487,39.64668970510144,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
["3 - 4",50.55987786728733,36.14846775822075,41.08106133964985,35.217242205338096,38.515873707121855,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
["4 - 5",38.887334475638255,33.21011929220768,34.56710738134416,27.905090653001565,35.38508932142025,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
["5 - 6",38.812198539112984,33.848932286255405,32.109422992428506,35.17903541676253,36.065738934725545,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[]
[]
[null,null,"Einspritzmengenberechnung"]
["max. Verbrauch 6.G",13.9,null,16.9,null,14.5]
["Motordrehungen / 100km",100089.68343480129,117081.29785488555,120983.19755245975,120682.31304028298,109884.81146191385,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
["Verbrauch pro Hub ml",0.0694377258623987,0,0.06984440956221197,0,0.06597818118396513,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
["spez.Gewicht Diesel",0.81,0.81,0.81,0.81,0.81,0.81,0.81]
["Einspr.Menge mg",56.244557948542955,0,56.5739717453917,0,53.44232675901176,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]

{"sheet":"Tabelle2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}

{"sheet":"Tabelle3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}