{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["LOG_3_8_11_Konstant_Diagramm"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"LOG_3_8_11_Konstant_Diagramm","index":0,"n_rows":30,"n_cols":16,"rows_kept":30,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["Monday",5,"April",2010,0.9262384259259259]
["038 906 012 H  ",null," 1.9l R4 EDC 0000SG  3332"]
[]
[null,"Group A:","'003",null,null,null,"Group B:","'008",null,null,null,"Group C:","'011"]
[null,null,"Engine speed","MAF (specified)","MAF (actual)","EGR duty cycle",null,"Engine speed","I.Q. Driver's req.","I.Q. via rpm(Torq)","I.Q. via air mass",null,"Engine speed","Specified MAP","Actual MAP","D.cycle MAP v."]
[null,"TIME","870-950 rpm","230-370 mg/H","230-370 mg/H","40-75%","TIME","rpm","40.0-42.0 mg/H","35.5-36.5 mg/H","36.0-39.0 mg/H","TIME","rpm","1850-1950 mbar","1700-2080 mbar","45-95%"]
["MARKER","STAMP"," /min"," mg/R"," mg/R"," %","STAMP"," /min"," mg/R"," mg/R"," mg/R","STAMP"," /min"," mbar"," mbar"," %"]
[null,0,2184,530,530,54.6,0.4,2205,17,48,27.6,0.8,2205,1315.8,1468.8,67.3]
[null,1.2,2226,505,485,51.8,1.6,2226,17,48,27.4,2,2247,1326,1438.2,65.3]
[null,2.4,2268,525,525,50.6,2.8,2289,17.8,48,28.8,3.23,2289,1346.4,1499.4,68.9]
[null,3.65,2310,525,520,55.8,4.06,2310,17.6,48,28.4,4.48,2331,1336.2,1489.2,71.3]
[null,4.88,2352,520,510,52.6,5.28,2352,17.6,48,28,5.68,2373,1336.2,1479,72.1]
[null,6.08,2373,520,530,53.8,6.48,2394,17.6,48,28.6,6.88,2415,1336.2,1479,74.9]
[null,7.31,2436,510,510,57.4,7.73,2436,17,48,27,8.14,2457,1305.6,1438.2,75.7]
[null,8.56,2457,485,485,57,8.97,2457,16,48,25.8,9.37,2478,1305.6,1377,74.9]
[null,9.78,2478,480,470,53.8,10.17,2499,15.2,48,25.8,10.57,2499,1275,1346.4,75.3]
[null,10.97,2499,460,470,58.2,11.37,2499,14.6,48,25,11.77,2520,1264.8,1315.8,74.9]
[null,12.17,2520,460,450,57.4,12.57,2520,14.6,48,24,12.97,2520,1264.8,1285.2,73.3]
[null,13.37,2520,455,455,53.8,13.77,2520,14.2,48,24.6,14.17,2541,1254.6,1275,73.7]
[null,14.57,2541,445,455,58.6,14.97,2541,11.4,48,24.4,15.37,2520,1183.2,1213.8,74.5]
[null,15.77,2541,400,375,57,16.17,2520,8.4,48,20.8,16.57,2520,1040.4,1111.8,46.6]
[null,16.97,2478,305,310,70.9,17.37,2457,0,48,16.6,17.77,2436,1030.2,1040.4,43.8]
[null,18.17,2373,305,270,63.4,18.57,2289,0,48,16.6,18.97,2205,1030.2,1020,34.7]
[null,19.37,2121,305,305,57.8,19.77,2037,0,48,16.6,20.17,1974,1020,1030.2,25.9]
[null,20.57,1911,305,315,56.2,20.97,1848,0,46.6,18.6,21.37,1806,1020,1030.2,24.7]
[null,21.77,1764,305,305,60.6,22.17,1722,0,45.2,18.8,22.57,1638,1020,1030.2,24.7]
[null,22.97,1554,305,295,61,23.37,1449,0,41,20.6,23.77,1029,1009.8,1020,24.7]
[null,24.17,945,310,365,57,24.57,903,0,30.8,24.6,24.97,903,999.6,999.6,25.1]
[null,25.37,903,310,320,63,25.77,903,0,30.8,24,26.17,903,999.6,999.6,24.7]
[null,26.6,903,310,315,62.2,27.02,903,0,30.8,24,27.44,903,999.6,989.4,25.1]