{"text_format":"2","workbook":"xls","n_sheets":6,"sheets":["Tabelle1","Ladedruck","Begrenz 1","Begrenz 2","Luftgrößen","Überblick"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Tabelle1","index":0,"n_rows":16,"n_cols":12,"rows_kept":16,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
[null,null,"Sunday",29,"May",2005,"20:47:18"]
[null,null,"038 906 019 DQ",null,"1.9l R4 EDC G000SG  1536"]
[]
["Group A:",null,null,"Group B:","'008",null,null,null,"'010"]
[null,"Intake Air Temp","Coolant Temp",null,"Engine speed","IQ driver's req","IQ via rpm(Torq)","IQ via MAF","MAF","Atmos. pressure","Intake air press.","Throttle"]
["TIME","~Amb.Temp.*C","~Amb.Temp.*C","TIME","2850-3150","65-70","47-51","47-60","900-1250","sensor -f96-","2100-2600",1]
["STAMP","°C","°C","STAMP"," /min"," mg/str"," mg/str"," mg/str"," mg/str"," mbar",null,"%"]
[0.36,47.7,90,0.8,1512,69.7,48,36.5,499.8,958.8,1205.1,100]
[1.68,47.7,90,2.12,1827,69.7,54.6,51.9,656.6,958.8,1497.6,100]
[3,48.6,90,3.44,2289,69.7,53.3,59.6,999.6,958.8,2246.4,100]
[4.32,49.5,90,4.76,2751,68.9,51.3,58.5,1087.8,958.8,2445.3,100]
[5.64,52.2,90,6.08,3150,67.3,50.2,56.5,1019.2,958.8,2293.2,100]
[6.96,55.8,90,7.4,3507,65.9,49.1,54.9,999.6,958.8,2328.3,100]
[8.28,61.2,90.9,8.72,3822,64.8,47.8,54.1,955.5,958.8,2351.7,100]
[9.6,66.6,90.9,10.04,4095,64,45.8,52.7,970.2,958.8,2316.6,100]
[10.92,72.9,90.9,11.36,4326,62.9,43.1,49.7,891.8,958.8,2246.4,100]

{"sheet":"Ladedruck","index":1,"n_rows":36,"n_cols":6,"rows_kept":36,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["Saturday",28,"May",2005,"21:40:41"]
["038 906 019 DQ",null,"1.9l R4 EDC G000SG  1536"]
[]
["Group A:","'011",null,null,"Tastverh","Ladedruck"]
[null,"rpm","Ladedruck","Ladedruck","Magnetventil","Ist"]
["TIME",null,"soll","Ist","35-80%","minus"]
["STAMP"," /min"," mbar"," mbar"," %","Soll"]
[0.01,1596,2060.4,1427.4,26.3,-633]
[0.44,1701,2131.8,1556.1,25.5,-575.7000000000003]
[0.88,1806,2203.2,1719.9,35.5,-483.2999999999997]
[1.32,1911,2264.4,1965.6,42.2,-298.8000000000002]
[1.76,2058,2305.2,2258.1,54.2,-47.09999999999991]
[2.2,2205,2325.6,2527.2,64.1,201.5999999999999]
[2.64,2373,2335.8,2574,65.7,238.19999999999982]
[3.08,2520,2346,2503.8,65.3,157.80000000000018]
[3.52,2667,2346,2433.6,64.9,87.59999999999991]
[3.96,2814,2346,2316.6,61.4,-29.40000000000009]
[4.4,2940,2346,2316.6,62.2,-29.40000000000009]
[4.84,3066,2346,2340,63,-6]
[5.28,3192,2335.8,2363.4,64.5,27.59999999999991]
[5.72,3297,2335.8,2363.4,65.7,27.59999999999991]
[6.16,3423,2335.8,2363.4,66.9,27.59999999999991]
[6.6,3528,2325.6,2363.4,68.1,37.80000000000018]
[7.04,3633,2315.4,2351.7,69.3,36.29999999999973]
[7.48,3738,2295,2340,70.5,45]
[7.92,3843,2274.6,2328.3,71.3,53.70000000000027]
[8.36,3927,2233.8,2304.9,72.9,71.09999999999991]
[8.8,4011,2203.2,2281.5,74.1,78.30000000000018]
[9.24,4095,2162.4,2246.4,75.7,84]
[9.68,4179,2121.6,2187.9,77.3,66.30000000000018]
[10.12,4242,2070.6,2152.8,78.5,82.20000000000027]
[10.56,4305,2029.8,2106,78.5,76.20000000000005]
[11,4347,1978.8,2059.2,79.3,80.39999999999986]
[11.44,4410,1938,2035.8,80.5,97.79999999999995]
[11.88,4431,1907.4,2000.7,81.7,93.29999999999995]
[12.31,4473,1887,1977.3,81.7,90.29999999999995]

{"sheet":"Begrenz 1","index":2,"n_rows":32,"n_cols":6,"rows_kept":32,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["Saturday",28,"May",2005,"21:17:18"]
["038 906 019 DQ",null,"1.9l R4 EDC G000SG  1536"]
[]
["Group A:","'008",null,null,null,"Ruß"]
[null,"rpm","Fahrer-","Drehmo-","Ruß-","minus"]
["TIME",null,"wunsch","Begrenz","begrenz","Drehmo"]
["STAMP"," /min"," mg/str"," mg/str"," mg/str"]
[0.35,1701,40.1,52.7,37.9,-14.800000000000004]
[0.79,1806,51.9,54.4,43.4,-11]
[1.23,1911,69.2,55.7,50.5,-5.200000000000003]
[1.66,2058,69.7,54.6,58.7,4.100000000000001]
[2.11,2205,69.7,53.5,59.6,6.100000000000001]
[2.55,2373,69.7,53,59.6,6.600000000000001]
[2.99,2520,69.7,52.2,59.3,7.099999999999994]
[3.43,2667,69.2,51.6,58.7,7.100000000000001]
[3.87,2814,68.6,51.3,58.5,7.200000000000003]
[4.31,2940,67.8,51.1,57.9,6.799999999999997]
[4.74,3087,67.5,50.5,57.4,6.899999999999999]
[5.18,3192,67,50,56.8,6.799999999999997]
[5.63,3318,66.7,49.7,56,6.299999999999997]
[6.07,3423,66.2,49.4,55.2,5.800000000000004]
[6.5,3549,65.9,48.9,48.9,0]
[6.94,3633,65.6,48.6,48.6,0]
[7.39,3738,65.1,48,48.3,0.29999999999999716]
[7.83,3843,64.8,47.5,47.5,0]
[8.26,3927,64.5,47.2,46.9,-0.30000000000000426]
[8.71,4011,64.2,46.9,46.7,-0.19999999999999574]
[9.14,4095,64,46.1,45.6,-0.5]
[9.53,4179,63.4,45,45.3,0.29999999999999716]
[9.97,4242,63.1,44.2,44.5,0.29999999999999716]
[10.41,4305,62.9,43.4,42.8,-0.6000000000000014]
[10.79,4347,62.6,42.3,41.7,-0.5999999999999943]

{"sheet":"Begrenz 2","index":3,"n_rows":46,"n_cols":5,"rows_kept":46,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["Saturday",28,"May",2005,"21:35:18"]
["038 906 019 DQ",null,"1.9l R4 EDC G000SG  1536"]
[]
["Group A:","'009"]
[null,"Engine speed","Injection Quantity","Inj. limit","Max IQ"]
["TIME","rpm","CC active","during a/t shift"]
["STAMP"," /min"," mg/str",null," mg/str"]
[0.43,1638,0,"  ",38.4]
[0.87,1743,0,"  ",41.5]
[1.31,1848,0,"  ",46.9]
[1.75,1953,0,"  ",52.7]
[2.19,2100,0,"  ",54.4]
[2.63,2247,0,"  ",53.3]
[3.07,2415,0,"  ",52.7]
[3.51,2562,0,"  ",52.2]
[3.95,2709,0,"  ",51.6]
[4.39,2835,0,"  ",51.1]
[4.83,2961,0,"  ",51.1]
[5.27,3087,0,"  ",50.5]
[5.71,3213,0,"  ",50]
[6.15,3318,0,"  ",49.7]
[6.59,3423,0,"  ",49.4]
[7.03,3528,0,"  ",49.1]
[7.47,3633,0,"  ",48.6]
[7.91,3738,0,"  ",48]
[8.35,3843,0,"  ",47.5]
[8.79,3927,0,"  ",47.2]
[9.23,4011,0,"  ",46.9]
[9.67,4074,0,"  ",46.1]
[10.11,4158,0,"  ",44.7]
[10.55,4221,0,"  ",43.4]
[10.99,4284,0,"  ",42]
[11.43,4326,0,"  ",40.6]
[11.87,4389,0,"  ",39.3]
[12.31,4431,0,"  ",37.9]
[167.61,903,0,"  ",26.4]
[168.05,903,0,"  ",25.8]
[168.49,903,0,"  ",26.1]
[168.93,903,0,"  ",26.4]
[169.37,903,0,"  ",26.1]
[169.81,903,0,"  ",25.8]
[170.25,903,0,"  ",26.1]
[170.69,903,0,"  ",26.4]
[171.13,903,0,"  ",26.6]
[171.57,903,0,"  ",26.4]
[172.01,903,0,"  ",26.1]

{"sheet":"Luftgrößen","index":4,"n_rows":30,"n_cols":5,"rows_kept":30,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["Saturday",28,"May",2005,"21:38:52"]
["038 906 019 DQ",null,"1.9l R4 EDC G000SG  1536"]
[]
["Group A:","'010","nichtssagend, da keine Drehzahl"]
[null,"Luft-","Umgeb.-","Lade-","Throttle"]
["TIME","masse","Druck","druck","Gaspedal"]
["STAMP"," mg/str"," mbar",null,"%"]
[0.01,490,958.8,1263.6,100]
[0.44,558.6,948.6,1357.2,100]
[0.88,597.8,958.8,1474.2,100]
[1.32,705.6,958.8,1638,100]
[1.76,823.2,958.8,1883.7,100]
[2.2,955.5,958.8,2223,100]
[2.64,1122.1,958.8,2538.9,100]
[3.08,1107.4,958.8,2562.3,100]
[3.52,1063.3,958.8,2492.1,100]
[3.96,975.1,958.8,2375.1,100]
[4.4,989.8,958.8,2304.9,100]
[4.84,975.1,948.6,2328.3,100]
[5.28,970.2,958.8,2351.7,100]
[5.72,975.1,958.8,2363.4,100]
[6.16,950.6,958.8,2375.1,100]
[6.6,935.9,958.8,2363.4,100]
[7.04,906.5,958.8,2340,100]
[7.48,872.2,958.8,2316.6,100]
[7.92,867.3,958.8,2281.5,100]
[8.36,837.9,948.6,2234.7,100]
[8.8,823.2,958.8,2187.9,100]
[9.24,793.8,958.8,2129.4,100]
[9.68,764.4,958.8,2082.6,100]

{"sheet":"Überblick","index":5,"n_rows":16,"n_cols":13,"rows_kept":16,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
[{"$nulls":4},"Sunday",29,"May",2005,"20:47:18"]
[{"$nulls":4},"038 906 019 DQ",null,"1.9l R4 EDC G000SG  1536"]
[]
["Group A:","'007",null,null,"Group B:","'008",null,null,null,"Group C:","'010"]
[null,"Fuel Temp","LLT","Wasser","rpm","Fahrer-","Drehmo-","Ruß-","Ruß",null,"Luftmasse","Ladedruck"]
["TIME","~Amb.Temp.*C",null,null,null,"wunsch","Begrenz","begrenz","minus","TIME",null,null,"Gaspedal"]
["STAMP","°C","°C","°C"," /min"," mg/str"," mg/str"," mg/str","Drehmo","STAMP"," mg/str",null,"%"]
[0.8,77.4,47.7,90,1512,69.7,48,36.5,-11.5,0.01,499.8,1205.1,100]
[2.12,77.4,47.7,90,1827,69.7,54.6,51.9,-2.700000000000003,1.24,656.6,1497.6,100]
[3.44,77.4,48.6,90,2289,69.7,53.3,59.6,6.300000000000004,2.56,999.6,2246.4,100]
[4.76,77.4,49.5,90,2751,68.9,51.3,58.5,7.200000000000003,3.88,1087.8,2445.3,100]
[6.08,77.4,52.2,90,3150,67.3,50.2,56.5,6.299999999999997,5.2,1019.2,2293.2,100]
[7.4,77.4,55.8,90,3507,65.9,49.1,54.9,5.799999999999997,6.52,999.6,2328.3,100]
[8.72,77.4,61.2,90.9,3822,64.8,47.8,54.1,6.300000000000004,7.84,955.5,2351.7,100]
[10.04,77.4,66.6,90.9,4095,64,45.8,52.7,6.900000000000006,9.16,970.2,2316.6,100]
[11.36,77.4,72.9,90.9,4326,62.9,43.1,49.7,6.600000000000001,10.48,891.8,2246.4,100]